{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"merged":[[0,0,0,7],[1,0,1,7],[2,0,2,7],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,3,6],[3,7,4,7],[45,0,45,7],[46,0,46,7]]}
["报价表"]
["报价单位（加盖公章）：                                                          年    月     日"]
["联系人：                                                        联系电话："]
["序号","物资/服务名称","规格或型号","数量","单位","金额（元，含税及运费）",null,"备注"]
[{"$nulls":5},"单价      ","总价     "]
[1,"吸顶灯","瓦数：36w；尺寸：直径375mm；色温：6500k",60,"盏"]
[2,"长条灯","吊装高度≦50cm，30cm*118cm LED平板灯，瓦数：58w；色温：6500k",94,"盏"]
[3,"平板灯","规格：LED60*60cm平板灯，瓦数：48W",3,"盏"]
[4,"壁装排气扇","335mm*335mm壁装百叶窗式连体换气扇，功率40W；封350mm*350mmPVC透气百叶出风口罩",35,"台"]
[5,"工业排气扇","350mm*350mm壁装排气扇；功率125W",1,"台"]
[6,"铝塑板","木龙骨+1.5cm阻燃板打底贴厚4.0mm铝塑板包柱子；含拆除旧铝塑板前后门框及拆除物外运处理。",30,"㎡"]
[7,"自动感应玻璃门","钢化玻璃厚度：12mm；含横梁及包304不锈钢板；含拆除旧铝合金玻璃门及拆除物外运处理等。",13,"㎡"]
[8,"感应门电机","无刷电机；遇阻立停、电子锁功能；支持门禁系统。",1,"台"]
[9,"感应门人脸机","产品尺寸：162.5mm×73mm×25mm；屏幕尺寸：4.5 英寸 LCD 触摸显示屏，分辨率1080×1920；设备容量：6000人脸 ；指纹容量：6000枚",1,"个"]
[10,"铝合金卷帘门","1.0mm厚铝合金卷帘门；含拆除旧卷帘门及拆除物外运处理。",13,"㎡"]
[11,"卷帘门电机","电机具有过热保护装置、遇阻立停功能",1,"台"]
[12,"铝合金卫生间门","拆除并清理旧木质卫生间门，安装铝合金卫生间门",3,"个"]
[13,"铝合金卫生间门","拆除并清理旧木质卫生间门，安装带自动闭门器铝合金卫生间门",2,"个"]
[14,"置物柜","尺寸：长120cm*宽35cm*高100cm，材质：铝蜂窝板",1,"个"]
[15,"铝扣板吊顶","拆除旧卫生间吊顶，重新安装集成吊顶。铝扣板规格：30cm*60cm厚0.6mm ；轻钢龙骨：国标38主骨+三角龙骨 +8mm吊杆 。",40,"㎡"]
[16,"集成吊顶灯","30*60cmLED灯",5,"套"]
[17,"台上盆","50cm*45cm洗手盆及下水管",2,"套"]
[18,"水龙头","立式单冷水龙头含软管及角阀",5,"套"]
[19,"吊顶拆除","拆除吊顶含拆除物外运处理",51,"㎡"]
[20,"复合地板","地面铺厚12mm复合地板，拆除旧地板含拆除物外运处理",51,"㎡"]
[21,"pvc踢脚线","6.5cm高pvc踢脚线",30,"m"]
[22,"2.5铜线布线","正负极两条2.5铜线+地线1.5铜线一条；地面套180°PVC防踩地线槽；墙面套PVC线槽及辅材、人工费。",60,"m"]
[23,"4.0铜线布线","正负极两条4.0铜线+地线1.5铜线一条含PVC线槽等辅材及人工费。",15,"m"]
[24,"1.5铜线布线","正负极两条1.5铜线含PVC线槽等辅材及人工费。",30,"m"]
[25,"配电箱","8路配电箱，含2p漏电保护器1个、1P20A空开3个。",1,"套"]
[26,"五孔插座","明装86型五孔插座",12,"个"]
[27,"屋顶防水","厚度：4mm；改性沥青底油+sbs沥青卷材",10,"㎡"]
[28,"顶棚刷白","天棚平板底满批粗底腻子粉一遍，内墙腻子粉3遍打磨刷环保型乳胶漆两遍。",51,"㎡"]
[29,"内墙乳胶漆","原墙面油漆空鼓、脱落、破损处铲除卫生清理后，破损处外墙腻子粉批补2遍后打磨并刷环保型乳胶漆两遍。",3400,"㎡"]
[30,"外墙真石漆","一、二层外墙高90cm墙跟，铲除破损腻子层，做透明防水涂料一遍，外墙腻子粉2遍打磨后刷真石漆专用底途、喷真石漆。并将拆除物外运处理。",165,"㎡"]
[31,"外墙真石漆","外墙墙跟90cm以上墙面搭门字架，表面卫生清理，墙面真石漆空鼓、脱落、破损处点补外墙腻子粉，打磨后刷真石漆专用底途、喷真石漆。",120,"㎡"]
[32,"侧面外墙油漆","搭门字架外墙面油漆空鼓、脱落、破损处铲除卫生清理后，做透明防水涂料一遍，外墙腻子粉2遍打磨后刷外墙涂料两遍。并将拆除物外运处理.",70,"㎡"]
[33,"外墙乳胶漆","搭门字架外墙面油漆空鼓、脱落、破损处铲除卫生清理后，点补外墙腻子粉，打磨后刷外墙涂料两遍。",360,"㎡"]
[34,"强弱电线路整理","2.4cm弧型线槽整理强弱电线路",300,"m"]
[35,"75寸电视","264Hz高刷模式4K 132Hz物理高刷屏",1,"台"]
[36,"超六类网络线","六类网络线套PVC管直径20mm电线管或2.4cm线槽。",1200,"m"]
[37,"16路硬盘录像机","1、产品可接入16路前端相机，具有2个SATA接口，可满配12TB硬盘 2、 设备支持文搜功能，可通过文字语义描述，快速检索目标对象或内容；内置16T硬盘。",1,"台"]
[38,"千兆交换机","1、设备可用千兆PoE电接口数量≥4，千兆电接口数量≥1，千兆光接口数量≥1，支持自适应802.3af/at供电标准，整机最大输出功率≥60W； 2、交换容量不小于14Gbps，转发性能不小于10.42Mpps。配400*300*160mm不锈钢防水箱。",1,"台"]
[39,"千兆POE交换机 ","1、设备可用千兆PoE电口数量≥8，千兆光口数量≥2，支持自适应802.3af/at供电标准，整机最大输出功率≥110W； 2、 交换容量不小于20Gbps，转发性能不小于14.88Mpps。配400*300*160mm不锈钢防水箱。",3,"台"]
[40,"400万全彩摄像机","1、设备最大图像尺寸≥2560 × 1440，且在2560x1440@25fps下，码率≤2Mbps，且清晰度不小于1400TVL，内置柔光灯，补光距离最远可达30 m，支持防补光过曝； 2、设备具有AI-ISP图像质量提升功能，在低照度环境下，可自动调节预览场景视频画面区域曝光、亮度、色彩饱和度等； 3、设备支持DC12V或POE供电。配支架。",15,"个"]
["合计：               元（含税及运费）"]
["注：报价应包含税金（增值税专用发票）、运费、卸车费、包工包料等一切费用。采用合计最低者中标。保修期为验收合格后1年，按实结算。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}